**LIST OF APPROVED BRAND NAMES**

All material specified in the schedule of quantities, specifications and conditions of contract must conform to the following brand names , be factory made and be of first quality, BIS /IS marked wherever available. Fabricated items shall be manufactured in accordance with the CPWD / ISI specifications and be first quality . Samples of all materials to be used must be submitted and got approved before actual procurement and Owner / Architect reserves the right to select any of the brand names specified herein for use.

|  |  |  |
| --- | --- | --- |
| S.No: | MATERIAL DESCRIPTION | BRAND / TRADE NAME OR EQUIVALENT APPROVED BY ENGINEER IN CHARGE |
| 1 | Paints | ASIAN, ICI, BERGER OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 2 | Water proof paint | APEX, WEATHER PROOF PAINT OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 3 | Locks | GODREJ, DORMA OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 4 | Terrazzo tiles (Paving) | EUROCON , SCORPIO, SIREX OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 5 | Ceramic tiles | KAJARIA, JOHNSON,ORIENT OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 6 | White Cement | BIRLA, J.K OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 7 | Ordinary  Portland Cement (43/53 Grade) | ULTRATECH, ACC, JK , CORAMANDAL, RAMCOOR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 8 | Steel Reinforcement Bars | TISCON,SAIL OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 9 | Structural steel sections | TISCO, SAIL OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 10 | Stone Aggregate( Blue/Black) | LOCALLY APPROVED OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 11 | Blocks/ Bricks & Brick Tiles | LOCALLY BEST AVAILABLE OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 12 | Anti Termite Treatment | PCI TERMEX OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 13 | Water Proof Shuttering Plywood | INDIAN PLYWOOD MFG.LTD, NATIONAL PLYWOOD, DURO, GREENPLY OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 14 | Teak Wood | 1ST CLASS BURMA TEAK OR GHANA TEAK , KERALA TEAK OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 15 | Flush Doors (ISI) | MAYUR/CENTURY/GREENPLY OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 16 | Rolling shutters | LOCALLY BEST AVAILABLE OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 17 | Laminates | SUNMICA/FORMICA/CENTURY/MERINO OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 18 | Water proofing | DR. FIXIT, CICO, DURA OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 19 | Aluminum Sections | HINDALCO, JINDAL OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 20 | Glass | SAINT GOBIN OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |
| 21 | Board & Ply | GREEN PLY, DURO, CENTURY, MERINO OR EQUIVALENT APPROVED BY ARCHITECT/CONSULTANT. |

Note:- For any other item required to be incorporated in work , sample shall be got approved from the Owner / Architect before actual procurement and commencement of that item of work.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  | **LIST OF APPROVED MAKE OR BRANDS W.B AND SANITARY WORK**  The Contractor shall quote for the best of the materials as specified below with ISI mark wherever applicable. he contractor shall obtain prior approval from the Employer/ Architects before placing order for the specific materials agencies. In case of non availability of any of the approved / specified materials / Agency. During the execution of the work, the Employers / Architects may approve suitable equivalent brand / agency and his decision shall be final and binding on the Contractor and the price variations. If any shall be adjusted accordingly.   * G.I Pipe and fittings : TATA/JINDAL with I.S marking on the body. * G.I Pipe for water supply : TATA/JINDAL with I.S marking on the body. * G.I soil, rainwater pipes   and fittings. : TATA/JINDAL with I.S marking on the body.   * G.I Sluice valves : TATA/JINDAL with I.S marking on the body. * Stone ware pipes : PERFECT or equivalent approved by Architect/consultant. * A.C pipes : Everest , Ramco or equivalent approved by   Architect/consultant.   * R.C.C pipes : Indane Hume pipe or equivalent approved by                                                                          Architect/consultant. * Brass & gun metal globe,   gate valves , feet valves : Leader, NETA or equivalent with I.S.I marking on the body.   * Sanitary fixtures : Hindustan Sanitary works, parryware , Neycer, Cera or ent                                                           equivalent having I.S.I mark on the body. * Water Supply, fancy fittings like   pillar taps, stop cocks, shower etc. : Essco, Jaguar or equivalent approved by Architect/consultant.   * C.P brass bib taps and stop cocks : I.S.I mark or tested as per Architect/consultants * Flush tank :Hindustan, Parryware with I.S.I mark or equivalent   approved by Architect/consultant.   * Storage Heaters : Racold, Spherehot, Venus or equivalent approved   by Architect/consultant.   * Fire Hydrant : Approved by Local Fire Brigade Authority. * Pumps : Kirloskar or equivalent Approved by Architect/consultant. * P.V.C pipes : Supreme or equivalent Approved by Architect/consultant. | |  |  |  |

**NOTE:**

1. In case of unavailability of any material of specific make an equivalent make can be used only after a written approval of Architect. The preference of make/brand of the material listed above will be decided by the Architect. The make/brand of any other item will be as mentioned in the drawings issued by the Architect.
2. The contractor shall provide samples of all materials mentioned in the list of makes as required by the Architect. A written approval of these samples shall be sought prior to commencement of any work. **Architect reserves the right to enquire the genuineness of any material used at site directly from the manufacturer/Dealer.**